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 4.Display And Function Instruction

	NO.
	symbols
	Explanation

	1
	[image: image1.png]



	Programming mode

	2
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	Manual mode

	3
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	When programming mode,it need set temperature,it can press “[image: image5.png]


”or “[image: image6.png]


” to adjust.Enter into temporary manual mode “[image: image7.png]


” and “[image: image8.png]


” flashing, when enter into next period“[image: image9.png]


” will disappear,thermostat run to the period of setting previously.

	4
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	Heating mode:relay connect,it will display “[image: image11.png]


” 
On power off state,when Anti-freezing function open,relay connect,it will display “[image: image12.png]


” 

	5
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	Cooling mode:relay connect,it will display“[image: image14.png]COOL



” 

	6
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	6 periods programming icon

	7
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	Timing on/off icon

	8
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	Room temperature

	9
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	Children lock:no any operation for 10 minutes,buttons will lock automatically,Press down button “[image: image20.png]


”for 3 seconds also can lock buttons,it will display lock icon on screen,unlock method:long press power button “[image: image21.png]


” for 3 seconds then move your finger.

	10
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	Windows open mode

	11
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	Clock setting icon


5.Quick Instruction Of Operation Icon
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6. Clock setting/Timing on/off setting.
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oN
OFF





Setting Screen

1) Clock Setting

Long press“[image: image26.png]


” for 3 seconds then enter setting screen,short press“[image: image27.png]


”to choose “[image: image28.png]EL;DK



” icon([image: image29.png]EL;DK



flashing),press “[image: image30.png]


” enter clock setting,it displays minute,hour,week, minute flashing then press “[image: image31.png]


” or “[image: image32.png]


” to adjust value. Press “[image: image33.png]


” to confirm and switch to next hour ,week setting,it is the same as minute setting.Press “[image: image34.png]


” button to save all time setting and return to previous screen.
2) Timing On/Off Setting 

Long press“[image: image35.png]


” for 3 seconds then enter setting screen,short press“[image: image36.png]


”to choose“[image: image37.png]


”([image: image38.png]


flashing) to set time of timing on;press “[image: image39.png]


” or “[image: image40.png]


” to adjust value.Press“[image: image41.png]


” to choose“[image: image42.png]OFF



” and set timing off.Cancel timing on/off:press ”[image: image43.png]


” to set [image: image44.png]


 as 00:00,press ”[image: image45.png]


” to set [image: image46.png]OFF



 as 00:00.It will quit automatically after setting finished 5 seconds,or press “[image: image47.png]


” button return to previous screen.
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3) 6 Periods Programming Mode Setting

4) Factory default periods programmable
[image: image54.png]



Programmable Plug In Thermostat





                         �      �      





1.Product Instruction


This is programming plug in thermostat,it is used for controlling air conditioner,carbon crystal heating panel,electric heating oven,heater and so on cooling heating devices,it is used conveniently and beautiful structure. 








2.Technical Data


Voltage:AC200~240V, 50HZ 


Load Current:16A(electric heating)


Temperature Control Precision:±0.5ºC                  


�
Temperature Setting Range:5ºC - 35ºC


Self Consumption Power:<1.5W             


Temperature Sensor:NTC�
�






Button Function Instruction  


NO.�
symbols�
Represent�
�
1�
��
Power On/Off�
�
2�
��
Selection Setting:short press to switch manual mode/programming mode;long press for 3 seconds to enter set clock and timing on/off.�
�
3�
��
Confirm Button/Enter Button, long press for 3 seconds to enter programming mode setting.�
�
4�
��
Increase Button,short press for increase value;long press for 3 seconds to enter advanced setting�
�
5�
��
Decrease Button, shortpress for decrease value;long press for 3 seconds to unlock�
�
6�
Indicator��
Light on is heating on,light off is heating off�
�






7.Advanced Setting(Suggest To Operate By Professional People)


Under power on state,press “�” for 3 seconds  to enter advanced setting,then press“�”to choose  option,press“�” or “�”to adjust value.To press“�” to next option.It will save setting and quit after setting finished 5 seconds.


No.�
Display�
Setting Option�
Data Setting Function�
Factory Default Setting�
�
1�
A1�
Windows open mode setting�
Press� to turn on, display 5℃(Trigger range of temperature: 5-25℃,Running time setting range: 5-60 minutes�
“�” means that the windows open mode is disable


Time dfault:15 minutes�
�
2�
A2�
Sensors Temperature Control Return Difference�
1-9ºC�
2ºC�
�
3�
A3�
Setting Temperature Highest Limit�
20-70ºC�
35ºC�
�
4�
A4�
Setting Temperature Lowest Limit�
1-10ºC�
5ºC�
�
5�
A5�
Measuring Temperature Calibration�
±5ºC(Display room temperature)�
0.5ºC Accuracy�
�
6�
A6�
Anti-freezing Function             �
00:Anti-freezing function close


01:Anti-freezing function open�
00:Anti-freezing function close�
�
7�
A7�
Power on/off state memory after electricity cut�
00:Thermostat off when electrify


01:Thermostat on/off with memory when electrify�
01�
�
8�
A8�
Working Mode�
00:Cooling Mode


01:Heating Mode�
01:Heating Mode�
�
9�
A9�
Programming Mode�
00:Enable Programming Mode


01:Disable Programming Mode�
00:Enable Programming Mode�
�
10�
AA�
Factory Setting�
88:it just display,no any meaning


00:Return to factory setting�
When it display "88", press � or �, then press �. When "00" appear,  it indicate that the thermostat is restored.�
�






Mode�
Explanation�
Printscreen�
�
Programming Mode�
Long press“�”,screen displays�(it means cycle control),screen displays “�” (it means Monday to Friday periods).See picture at right:first period flashing,press “�” or “� ”to adjust setting temperature,press “�” to adjust clock,press “�”to next period setting,same like this to finish 6 periods setting,then press “�”, screen displays “�”and “�” (Saturday and Sunday),set it as per previous method,it will save and quit after setting finished 5 seconds.�
�


��
�
Note1.the usage of temporary manual mode:


When thermostat is in programming mode,such as current time is 16:00,thermostat will set corresponding room temperature(factory setting is 15ºC) as per current period(factory setting afternoon going out period is 12:30-17:30),if current day you end work 1 hour earlier,(16:30 is 1 hour earlier than 17:30),you can press increase/decrease button temporarily to modify temperature to the temperature you wanted(such as 20ºC),then the thermostat will keep the room temperature in 20ºC until next period,no any operation,thermostat will run the setting temperature (thermostat default 20ºC) automatically of afternoon entering room period(17:30-22:00) at 17:30.





Period�
Icon�
Default Time�
Default Temperature�
�
Working Day�
1�
��
06:00�
20℃�
�
�
2�
��
08:00�
15℃�
�
�
3�
��
11:30�
15℃�
�
�
4�
��
12:30�
15℃�
�
�
5�
��
17:30�
20℃�
�
�
6�
��
22:00�
15℃�
�
Weekend�
1�
��
08:00�
20℃�
�
�
2�
��
23:00�
15℃�
�
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